**Aurora Lighting – AR-5 & AR-6 Trim Installation**

1. Always properly isolate the fixture from its power source before performing any maintenance.
2. Remove existing lamp and trim.
3. Clip the lamp holder into the lamp holder bracket.
4. Squeeze the torsion springs together and insert springs into the spring tabs inside the fixture housing.
5. Firmly push the trim up to properly seat the trim in the fixture housing.
6. Gently push the insert (baffle or cone) into the trim until it seats properly.
7. Install new Aurora LED retrofit lamp.